|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Project  |  |  PCN |  | County |  | Contractor |  |
|  |
| Weigher Signature |  |  |  |
|  |
| InitialsContractor/Engineer | Date(m/d/y) | Time of balance for zero load of bucket | Gross Weight of truck from Certified Scale(Lb) | TareWeight(Lb) | Net Weight(Lb) | \* 1.0% of Net Weight from Certified Scale(Lb) | Net Weight loaded from Loader Scale(Lb) |
| AM | PM |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |

\* Net Weight obtained with the loader scale shall be within 1.0% of the net weight obtained from the certified scale.

Zero Weight of Bucket – Performed by the operator at a minimum of twice daily.

Accuracy Test – Performed at a minimum once per week